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Estimated assembly time: 30 minutes (2 people)











[image: ]
Step by step Assembly Instructions

TOOLS REQUIRED                                                                       PART LIST
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POZIDRIV SCREWDRIVER X 1				 PLASTIC LEGS X 16 		SCREWS X 16

FITTING LEGS INSTRUCTION
[image: ]1.  Spread the removed packing material on the floor to damage to the unit. 
2.  Place the unit on its back on the packing material.
[image: ]3.  At the corners of unit locate the pilot holes for the leg fixing screw.
4. Align the legs with the individual pilot holes.
5. Insert a screw supplied through the hole in the leg and into the pilot hole.
[image: ]6. Tighten the screws with a pozidrive screwdriver, see image below.
7. Carefully turn the unit over without dropping it so the legs are on the floor
8. Carefully lift and carry the unit into its location, 
DO NOT DRAG!







Join your elements together using the spring loaded latches.
[image: ]
Position your elements as you want it configured, leaving a 1-foot gap between each piece. Feel along the bottom and pull out the latches on each side. 

Step 1: Pull out the latch.
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Step 2: Line up the latch with the adjacent catch bracket.
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Step 3: Push the two furniture elements together, listening for a clicking sound, until the two pieces are touching.
[image: ]

Step 4: If your unit doesn’t include a Right corner section, remove the pull out bracket from the Middle section.
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If you want to move your unit.
To separate the pieces lift the Right hand unit to release the brackets.
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Storing separate elements safely.
Turn the latches so that they fully under the furniture piece.
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	FOR PARTS & TECHNICAL SUPPORT VISIT:
Telephone:
01924950108
Email Address:
support@bedkingdom.co.uk
	Manufacturer
Flair Furnishings Ltd t/a Bedkingdom,
Old Delivery Office, Oldfield Lane,
Heckmondwike, England, WF16 0JD
Support@bedkingdom.co.uk
01924 950108
	EU Responsible (for authorities only)
eucomply OÜ
Pärnu mnt 139b-14
11317 Tallinn, Estonia
hello@eucompliancepartner.com
+3375690241
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IMPORTANT! KEEP FOR FUTURE REFERENCE

SOLACE+CO
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SOLACE+CO care Instructions

Please periodically check all fittings and re-tighten as necessary.
Upholstered fumiture should not be exposed to direct sunlight for long periods.

Please do not place your upholstery in direct contact with a strong heat source. Leave a 30cm gap between upholstery and
radiators.

Please do not allow children to jump up and down on the upholstery.

Avoid allowing pets on the upholstery as their claws may cause damage to the fabric.

Avoid sitting on the arms of the upholstery o on the front edge of the seat s this can compress the foam and damage the
frame of your upholstery causing premature wear and distortion.

When your new sofa arrives, you may notice that some of the seating or back padding may have been creased or squashed
during transit. This can be simply corrected by gently patting back into shape to re-distribute the filing and reshape the
covering.

Our fixed cover fabric sofas can be cleaned by using water and a neutral soap to remove stains. Always apply the treatment
to a concealed area first to test for colourfastness

Light vacuuming of the sofa wil help to prolong the life of the covers. Be very careful, as some vacuum attachments have
sharp edge that could damage your sofa.

In the unfortunate event of severe staining on the fabric, take expert advice from a specialist upholstery cleaning
company before attempting to clean or remove the stain.




